

During the MSI install you input comment separated values (csv) such as D1,D2,D3 to specify three device. 

It automatically generates an agent.cfg file and THIS MSI generates an generic Mazak Devices.xml file (for each device too) and installation time.

The D1,D2,D3 are put into the Agent.cfg file:

Devices = Devices.xml

ServiceName = MTConnectAgent

Port = 5001

CheckpointFrequency=10000

AllowPut=true

Adapters

{

**D1**

**{**

**Host = 127.0.0.1**

**Port = 7878**

**}**

**D2**

**{**

**Host = 127.0.0.1**

**Port = 7879**

**}**

**D3**

**{**

**Host = 1270.0.01**

**Port = 7880**

**}**

}

# Logger Configuration

logger\_config

{

logging\_level = fatal

output = cout

}

And the devices.xml file is installed by creating D1, D2, D3 devices:



Renames have changed. Here is the latest mapping:

[TAGRENAMES]

# Revision 8 2018 for TechSolve Agent

X\_actual=Xabs

Y\_actual=Yabs

Z\_actual=Zabs

# p1 is controller 1!!

P1S1\_speed\_act=Srpm

p1\_execution=execution

p1\_program=program

p1\_feedrate\_override=path\_feedrateovr

p1\_feedrate\_act=path\_feedratefrt

p1\_spindle\_override=Sovr

p1\_program=program

p1\_mode=controllermode

[ENUMREMAPPING]

p1\_execution.READY=IDLE

p1\_execution.ACTIVE=EXECUTING

p1\_execution.INTERRUPTED=PAUSED

p1\_execution.STOPPED=PAUSED